**Site rehabilitation and hole capping**

**Purpose:**

* To ensure drill sites are left clean and safe after moving off the drill pad
* To ensure that holes are kept free of debris and to mark the actual drill hole point

**Steps for Rehab:**

* Clean up any oil spills and rubbish on site
* Contaminated soil to be removed bagged and taken off site
* Sump fluids to be pumped downhole if possible or additional sumps to be dug to share equal to avoid overflow when back filling.

**DO NOT PUMP SUMP FLUIDS DOWNHOLE IF CONTAMINATED WITH OIL.**

* Level the site
* Inspect site after rehab. Responsible persons: Safety Officer, Supervisor and Site Manager
* All rubbish to be collected from site and taken back to camp for proper disposal.

**DO NOT DUMP RUBBISH IN THE SUMPS OR IN THE BUSH.**

**Capping of holes:**

* Holes will be capped with cement blocks.
* Cement block measurements: 50cmx50cmx20cm
* To be dug in level with the ground.
* Use suitable tool to scribe below information onto blocks:
  + Hole numbers
  + E.O.H depth
  + Azimuth
  + Angle

**JHA:**

PPE (Gloves; glasses; Hard hat; safety boots)